{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":false,"merged":[[7,2,7,4],[9,2,9,4],[36,2,36,4],[42,3,42,11],[43,2,43,13],[9,7,9,9],[8,5,8,9],[43,0,43,1],[40,7,41,14],[6,0,6,4],[6,5,6,9],[6,10,6,14],[7,10,7,11],[34,13,34,14],[36,7,36,8],[39,7,39,14],[7,12,7,14],[8,12,8,14],[9,12,9,14],[10,12,10,14],[10,10,10,11],[8,10,8,11],[9,10,9,11],[8,0,8,4],[12,0,12,2],[12,4,12,7],[12,10,12,12],[18,8,18,14],[32,0,32,6],[32,7,32,14],[33,2,33,6],[33,0,33,1],[36,0,36,1],[34,0,34,1],[35,0,35,2],[35,3,35,6],[34,9,34,10],[37,2,37,6],[39,5,39,6],[36,9,36,14],[35,9,35,14],[35,7,35,8],[38,7,38,14],[38,2,38,6],[37,9,37,14],[38,0,38,1],[39,0,39,1],[40,2,40,3],[41,2,41,6],[40,0,40,1],[41,0,41,1],[39,3,39,4],[37,0,37,1],[26,8,26,13],[1,5,2,14],[27,8,27,11],[28,8,28,11],[29,8,29,11],[11,0,11,14],[3,5,3,14],[4,5,4,14],[25,8,25,14],[24,8,24,14],[14,8,14,14],[15,8,15,14],[16,8,16,14],[22,8,22,14],[17,8,17,14],[21,8,21,14],[19,8,19,14],[20,8,20,14],[34,11,34,12],[33,10,33,14],[10,0,10,4],[7,5,7,9],[10,7,10,8],[34,4,34,6],[34,2,34,3],[13,0,18,7],[30,8,30,11],[23,8,23,14]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":5},"DMFV Schallmessung"]
[]
[{"$nulls":5},"gemäß Auszug aus der Lärmvorschrift für Luftfahrzeuge (LVL)"]
[{"$nulls":5},"vom 1. August 2004"]
[]
["Modelleigner / Verein",{"$nulls":4},"Messort",{"$nulls":4},"Messbeauftragter"]
["Eigentümer:",{"$nulls":9},"Name:"]
[{"$nulls":10},"Vorname:"]
["Verein:",{"$nulls":4},"Datum:",{"$nulls":4},"Straße:"]
[{"$nulls":5},"Messzeit:",null,null,null,"Uhr","PLZ, Ort:"]
["Klima und Wetter:"]
["Niederschlag:",null,null,"nein","Windgeschwindigkeit: ",{"$nulls":4},"[m/s]","Temperatur:",null,null,null,"°C"]
["hier könnte ein Bild des Modells hin"]
[{"$nulls":8},"Referenzbedingungen nach der LVL"]
[{"$nulls":8},"Anordnung der Messpunkte in ca. 1,0 m Höhe über einem kurz gemähten Grasboden"]
[{"$nulls":8},"Flugmodell in 1m Höhe, Flugzeuglängsachse parallel zum Boden u. 90° ± 30° zur Windrichtung"]
[{"$nulls":8},"Betriebszustand: Schwebeflug"]
[{"$nulls":8},"keine Reflexionen verursachende Gegenstände im Umkreis von 30 m (Modell u. Messgerät)"]
[{"$nulls":8},"Messgröße: LAmax in dB(A), Betriebsart slow"]
[{"$nulls":8},"LAmax (25m) = arithmetischer Mittelwert der Messwerte an Messpunkt 1-3"]
[{"$nulls":8},"Messdauer pro Messpunkt min. 30 Sek"]
[{"$nulls":8},"Umgebungstemperatur zwischen 10° und 30° C"]
[{"$nulls":8},"Umgebungsgeräusch mindestens 10 dB(A) unter dem des Modells"]
[{"$nulls":8},"Windgeschwindigkeit <= 5m/sec."]
[{"$nulls":8},"kein Niederschlag"]
[{"$nulls":8},"Schalldruckpegel LAmax in dB(A)"]
[{"$nulls":8},"   1. Messpunkt",{"$nulls":4},"dB(A)"]
[{"$nulls":8},"   2. Messpunkt",{"$nulls":4},"dB(A)"]
[{"$nulls":8},"   3. Messpunkt",{"$nulls":4},"dB(A)"]
[{"$nulls":8},"   LAmax 25m =",null,null,null,0,"dB(A)"]
[]
["Modelldaten",{"$nulls":6},"verwendete Messgeräte"]
["Modellname:",{"$nulls":6},"Schallpegelmesser:"]
["Gewicht: (kg)",null,null,null,"(max. Startmasse)",null,null,"Klasse:",null,"kalibriert am: ",null,null,null,"(min. alle 2 Jahre)"]
["Motorhersteller / Bez.:",{"$nulls":6},"Windmesser:"]
["Motortyp:",{"$nulls":5},"ccm","Thermometer:"]
["Rotorblätter:",{"$nulls":6},"Bemerkungen:"]
["Material:",null," "]
["Blattzahl:"]
["max. Drehzahl:",null,null,null,"[1/min]",null,null,"Unterschrift Messbeauftragter"]
["Schalldämpfer:"]
[null,null,null,"Dieser Messbericht kann als Lärmpass verwendet werden"]
["Hinweis:",null,"Die Daten der gelb hinterlegten Felder müssen im Lärmpass enthalten sein"]